(footprint "TL3301SPF160QG" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 0)
  (attr smd)
  (fp_text reference "REF**" (at 0 -0.5 unlocked) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp dcfc0eb7-b408-4d38-8783-7830e776bab5)
  )
  (fp_text value "TL3301SPF160QG" (at 0 1 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp b862ae5f-d2c9-4838-b8f1-3f7597ce06e1)
  )
  (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 2bbe75d4-f478-4f3a-a4bf-31c46b133690)
  )
  (fp_rect (start -3 -3) (end 3 3) (layer "F.SilkS") (width 0.12) (fill none) (tstamp f41f2837-a81c-4d37-8188-c38cf3c775d8))
  (fp_rect (start -3 -3) (end 3 3) (layer "F.Fab") (width 0.12) (fill none) (tstamp b53658c8-1cb4-4c08-a8e1-adeb7b9a6f15))
  (pad "1" smd roundrect (at -4.5 2.25) (size 3 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp dcc60922-4d9c-4103-b820-2ac395a00d24))
  (pad "2" smd roundrect (at 4.5 2.25) (size 3 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp 3ad4040f-38a8-49f6-9fbb-8424ec87ba69))
  (pad "3" smd roundrect (at -4.498165 -2.25) (size 3 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp dd930aca-fb73-4875-b380-a8b82323117e))
  (pad "4" smd roundrect (at 4.5 -2.25) (size 3 1.524) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25) (tstamp c0518513-56e7-460f-9b4f-fb8e7fe6e423))
)
