(kicad_pcb (version 20211014) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "EN")
  (net 2 "GND")
  (net 3 "Net-(J1-PadA1_B12)")
  (net 4 "Net-(J1-PadA4_B9)")
  (net 5 "unconnected-(J1-PadA5)")
  (net 6 "unconnected-(J1-PadA6)")
  (net 7 "unconnected-(J1-PadA7)")
  (net 8 "unconnected-(J1-PadA8)")
  (net 9 "unconnected-(J1-PadB5)")
  (net 10 "unconnected-(J1-PadB6)")
  (net 11 "unconnected-(J1-PadB7)")
  (net 12 "unconnected-(J1-PadB8)")
  (net 13 "Net-(J1-PadS1)")
  (net 14 "+3.3V")
  (net 15 "unconnected-(U1-Pad4)")
  (net 16 "unconnected-(U1-Pad5)")
  (net 17 "unconnected-(U1-Pad6)")
  (net 18 "unconnected-(U1-Pad7)")
  (net 19 "unconnected-(U1-Pad8)")
  (net 20 "unconnected-(U1-Pad9)")
  (net 21 "unconnected-(U1-Pad10)")
  (net 22 "unconnected-(U1-Pad11)")
  (net 23 "unconnected-(U1-Pad12)")
  (net 24 "D-")
  (net 25 "D+")
  (net 26 "unconnected-(U1-Pad15)")
  (net 27 "unconnected-(U1-Pad16)")
  (net 28 "unconnected-(U1-Pad17)")
  (net 29 "unconnected-(U1-Pad18)")
  (net 30 "unconnected-(U1-Pad19)")
  (net 31 "unconnected-(U1-Pad20)")
  (net 32 "unconnected-(U1-Pad21)")
  (net 33 "unconnected-(U1-Pad22)")
  (net 34 "unconnected-(U1-Pad23)")
  (net 35 "unconnected-(U1-Pad24)")
  (net 36 "unconnected-(U1-Pad25)")
  (net 37 "unconnected-(U1-Pad26)")
  (net 38 "IO0")
  (net 39 "unconnected-(U1-Pad28)")
  (net 40 "unconnected-(U1-Pad29)")
  (net 41 "unconnected-(U1-Pad30)")
  (net 42 "unconnected-(U1-Pad31)")
  (net 43 "unconnected-(U1-Pad32)")
  (net 44 "unconnected-(U1-Pad33)")
  (net 45 "unconnected-(U1-Pad34)")
  (net 46 "unconnected-(U1-Pad35)")
  (net 47 "RX0")
  (net 48 "TX0")
  (net 49 "unconnected-(U1-Pad38)")
  (net 50 "unconnected-(U1-Pad39)")

  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 16b33fd6-47ea-4b5b-9059-35418c8faa63)
    (at 120.142 95.504)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "main jednotka.kicad_sch")
    (property "Sheetname" "")
    (path "/d97b81db-4627-4783-9b6f-b318a4374236")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.68) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4f8a0e86-11a0-4e2e-8d96-0ea217bd6442)
    )
    (fp_text value "470nF" (at 0 1.68) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cef6ee29-f938-46c9-b73f-d0bc9c1be849)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp a3bcd283-2c61-4cee-9adc-38ad2fd04402)
    )
    (fp_line (start -0.261252 -0.735) (end 0.261252 -0.735) (layer "F.SilkS") (width 0.12) (tstamp adae7b39-cade-4ce5-a495-025eced731cd))
    (fp_line (start -0.261252 0.735) (end 0.261252 0.735) (layer "F.SilkS") (width 0.12) (tstamp f11d956b-db3e-474a-8271-c14f95e7d17a))
    (fp_line (start -1.7 -0.98) (end 1.7 -0.98) (layer "F.CrtYd") (width 0.05) (tstamp 27bbe7cd-0452-4d18-bcf5-a4b63b818980))
    (fp_line (start 1.7 0.98) (end -1.7 0.98) (layer "F.CrtYd") (width 0.05) (tstamp 70a90805-cac8-457d-9e2d-58357ad9e743))
    (fp_line (start -1.7 0.98) (end -1.7 -0.98) (layer "F.CrtYd") (width 0.05) (tstamp 848cd766-8bbe-45a4-8c96-39c460b483c9))
    (fp_line (start 1.7 -0.98) (end 1.7 0.98) (layer "F.CrtYd") (width 0.05) (tstamp b54561ed-60d7-41f7-9df3-0f5ba99ce91b))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 7f57762d-3a24-4a74-ba9e-e34efbed5eb4))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp ab833d7f-2a9b-4c77-9e80-e0d844c9558e))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp c68fcddb-602b-4adb-ac47-734d5dbf15b2))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp cf09ddae-3014-477c-a516-5973bb754387))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "EN") (pintype "passive") (tstamp 30319586-a95c-49d1-b944-0732bb290fee))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive") (tstamp 92661873-0df7-4439-b845-55a81d6a5425))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE) (tstamp 4b3f78ee-0157-4199-bdf0-983598125604)
    (at 141.292 77.404)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "main jednotka.kicad_sch")
    (property "Sheetname" "")
    (path "/e145f402-c81b-4d2e-8282-9839c39c39f7")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4ae8cd24-1eef-4c0d-9f8e-10924450fa97)
    )
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5f13289b-543d-4d87-87ba-278e3a69801d)
    )
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
      (effects (font (size 0.5 0.5) (thickness 0.08)))
      (tstamp 79928532-7b84-4b2e-bbe3-40bddfabc7be)
    )
    (fp_line (start -0.227064 -0.735) (end 0.227064 -0.735) (layer "F.SilkS") (width 0.12) (tstamp 2be2bab8-0d61-4cd4-86fe-d0150fd23aab))
    (fp_line (start -0.227064 0.735) (end 0.227064 0.735) (layer "F.SilkS") (width 0.12) (tstamp 76366915-5e68-4719-8d89-a750944857d3))
    (fp_line (start 1.68 0.95) (end -1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 2e894aa2-c6b9-40d0-9d96-d3686c5e48cd))
    (fp_line (start 1.68 -0.95) (end 1.68 0.95) (layer "F.CrtYd") (width 0.05) (tstamp 3cc05a5c-9029-4577-b252-470fd8bd8994))
    (fp_line (start -1.68 0.95) (end -1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 7eae017b-9c53-4f89-a75c-7d7bca1508cb))
    (fp_line (start -1.68 -0.95) (end 1.68 -0.95) (layer "F.CrtYd") (width 0.05) (tstamp 83ca5a3a-75cc-4185-9068-adbd3a62df51))
    (fp_line (start -1 0.625) (end -1 -0.625) (layer "F.Fab") (width 0.1) (tstamp 63775f65-a36f-4b4d-a5f8-b16ce0722eee))
    (fp_line (start 1 -0.625) (end 1 0.625) (layer "F.Fab") (width 0.1) (tstamp 8c170416-2993-4d35-a651-1fa97f05dac5))
    (fp_line (start -1 -0.625) (end 1 -0.625) (layer "F.Fab") (width 0.1) (tstamp f541e696-26a4-441c-ad8c-7a15823af8ab))
    (fp_line (start 1 0.625) (end -1 0.625) (layer "F.Fab") (width 0.1) (tstamp fc94786f-3d49-44c4-b284-ed1929c9220b))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 14 "+3.3V") (pintype "passive") (tstamp 5d4a0694-f728-4f2c-841c-237e55435c32))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "EN") (pintype "passive") (tstamp 86b3260b-5f9d-4d8b-938d-51c68a45bdb9))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "esp32S3:XCVR_ESP32-S3-WROOM-1-N16R2" (layer "F.Cu")
    (tedit 63D5066D) (tstamp c91f7b89-dfb8-4109-a5fe-a0ca7b1e5a41)
    (at 128.817 79.974)
    (property "MANUFACTURER" "Espressif")
    (property "MAXIMUM_PACKAGE_HEIGHT" "3.25mm")
    (property "PARTREV" "v1.0")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "main jednotka.kicad_sch")
    (property "Sheetname" "")
    (path "/a8b02476-d683-432d-968b-46ff0d122014")
    (attr smd)
    (fp_text reference "U1" (at -6.575 -14.135) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e3ae00f0-4816-419d-a5ec-72cce332e06b)
    )
    (fp_text value "ESP32-S3-WROOM-1-N16R2" (at 7.395 14.365) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 9c762782-2e37-4f8f-b4bd-0a248f8c8ece)
    )
    (fp_text user "ANTENNA" (at -4.5 -9.5) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8dbaa447-b0b3-4aa4-a881-9bfbf0ebc1b6)
    )
    (fp_line (start -9 -12.75) (end 9 -12.75) (layer "F.SilkS") (width 0.127) (tstamp 1061b8b9-0668-4ba8-8e36-76f7a764ed82))
    (fp_line (start -9 12.75) (end -7.755 12.75) (layer "F.SilkS") (width 0.127) (tstamp 167d8a05-a17a-4b53-a5fa-e10672c3b810))
    (fp_line (start 9 -12.75) (end 9 -6.03) (layer "F.SilkS") (width 0.127) (tstamp ab49e99d-815a-40f2-8416-7e97af6252dd))
    (fp_line (start 9 12.75) (end 7.755 12.75) (layer "F.SilkS") (width 0.127) (tstamp d3f6f4de-0bd0-4bc1-85f8-96744b9bed49))
    (fp_line (start -9 -6.03) (end -9 -12.75) (layer "F.SilkS") (width 0.127) (tstamp e4a936eb-e6ee-4dcf-8f8b-9cbceedc745c))
    (fp_line (start -9 12.02) (end -9 12.75) (layer "F.SilkS") (width 0.127) (tstamp e52e309f-a821-49fd-a18e-80ecf4022e8a))
    (fp_line (start 9 12.02) (end 9 12.75) (layer "F.SilkS") (width 0.127) (tstamp f3724147-1fdf-4fa3-a40b-f19cea47970d))
    (fp_circle (center -10.2 -5.26) (end -10.1 -5.26) (layer "F.SilkS") (width 0.2) (fill none) (tstamp 1fd0d8d3-b202-472d-81fe-82922eb88229))
    (fp_line (start -9.75 13.5) (end 9.75 13.5) (layer "F.CrtYd") (width 0.05) (tstamp 759e0326-e4da-497b-8e68-b4b76455177d))
    (fp_line (start -9.75 -13) (end 9.75 -13) (layer "F.CrtYd") (width 0.05) (tstamp a2a7b43c-0c87-4efb-bf60-1f67f2ea7763))
    (fp_line (start -9.75 13.5) (end -9.75 -13) (layer "F.CrtYd") (width 0.05) (tstamp bcafa36b-74ea-4b8b-8daa-8674cdac9640))
    (fp_line (start 9.75 -13) (end 9.75 13.5) (layer "F.CrtYd") (width 0.05) (tstamp ed86218b-4e62-4998-8d69-6d971495874d))
    (fp_line (start 9 12.75) (end -9 12.75) (layer "F.Fab") (width 0.127) (tstamp 140070b9-23f9-40e7-87ec-f1c7b815ca4d))
    (fp_line (start 9 -6.75) (end 9 12.75) (layer "F.Fab") (width 0.127) (tstamp 71e0de75-fe25-4a30-843e-1ea3b2aa5e15))
    (fp_line (start -9 12.75) (end -9 -6.75) (layer "F.Fab") (width 0.127) (tstamp 8cd4a4ce-9c82-4e46-bb9b-72e28c27fc38))
    (fp_line (start -9 -6.75) (end -9 -12.75) (layer "F.Fab") (width 0.127) (tstamp 8ea5d03a-08a1-4ab3-bbc0-b542fac9267c))
    (fp_line (start -9 -12.75) (end 9 -12.75) (layer "F.Fab") (width 0.127) (tstamp a52cbe97-8d84-4b5a-97a1-784af50bac90))
    (fp_line (start 9 -12.75) (end 9 -6.75) (layer "F.Fab") (width 0.127) (tstamp e1832efa-5f8f-406f-ada1-088ec2d8ccb7))
    (fp_line (start -9 -6.75) (end 9 -6.75) (layer "F.Fab") (width 0.127) (tstamp eed68711-92f4-4937-8e8a-3613f931cc4c))
    (fp_circle (center -10.2 -5.26) (end -10.1 -5.26) (layer "F.Fab") (width 0.2) (fill none) (tstamp ebedde65-8a2c-4455-a8fe-e60bcae59ab6))
    (pad "1" smd rect (at -8.75 -5.26) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 5959fd7a-c356-4f0f-86a3-616a939c9cef))
    (pad "2" smd rect (at -8.75 -3.99) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "+3.3V") (pinfunction "3V3") (pintype "power_in") (tstamp cbf36341-9920-4815-8b07-9d0355d17f39))
    (pad "3" smd rect (at -8.75 -2.72) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "EN") (pinfunction "EN") (pintype "input") (tstamp e09157b7-7613-465a-8804-29fc56198128))
    (pad "4" smd rect (at -8.75 -1.45) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "unconnected-(U1-Pad4)") (pinfunction "IO4") (pintype "bidirectional+no_connect") (tstamp 150b7722-6c79-4021-8e1f-7358975e9159))
    (pad "5" smd rect (at -8.75 -0.18) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "unconnected-(U1-Pad5)") (pinfunction "IO5") (pintype "bidirectional+no_connect") (tstamp c5a8cba8-0c9d-4b18-bba3-5063aa96c048))
    (pad "6" smd rect (at -8.75 1.09) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "unconnected-(U1-Pad6)") (pinfunction "IO6") (pintype "bidirectional+no_connect") (tstamp e3ab160e-d884-426f-9722-a13873399c3f))
    (pad "7" smd rect (at -8.75 2.36) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "unconnected-(U1-Pad7)") (pinfunction "IO7") (pintype "bidirectional+no_connect") (tstamp 951feab5-0e50-49aa-ba86-d9c43fe2a372))
    (pad "8" smd rect (at -8.75 3.63) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "unconnected-(U1-Pad8)") (pinfunction "IO15") (pintype "bidirectional+no_connect") (tstamp 1d46fdd6-8c69-4d59-8805-6e59ab48167e))
    (pad "9" smd rect (at -8.75 4.9) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "unconnected-(U1-Pad9)") (pinfunction "IO16") (pintype "bidirectional+no_connect") (tstamp 8838b859-fa2e-4b81-9c2c-08a60afdb63c))
    (pad "10" smd rect (at -8.75 6.17) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "unconnected-(U1-Pad10)") (pinfunction "IO17") (pintype "bidirectional+no_connect") (tstamp 2a59cdb7-a33b-4696-a4a6-d3de4c16fcba))
    (pad "11" smd rect (at -8.75 7.44) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "unconnected-(U1-Pad11)") (pinfunction "IO18") (pintype "bidirectional+no_connect") (tstamp 4ab1af11-c438-42ac-bc7c-581281a54793))
    (pad "12" smd rect (at -8.75 8.71) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "unconnected-(U1-Pad12)") (pinfunction "IO8") (pintype "bidirectional+no_connect") (tstamp 708403eb-5333-46a7-8d81-e9516b1a811b))
    (pad "13" smd rect (at -8.75 9.98) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "D-") (pinfunction "IO19") (pintype "bidirectional") (tstamp 8af1f5d1-2a27-4f73-8787-e6bcbb9a2a35))
    (pad "14" smd rect (at -8.75 11.25) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "D+") (pinfunction "IO20") (pintype "bidirectional") (tstamp 1f9f2bfd-617a-4568-a04f-8f2bfee9fbfc))
    (pad "15" smd rect (at -6.985 12.5) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "unconnected-(U1-Pad15)") (pinfunction "IO3") (pintype "bidirectional+no_connect") (tstamp 791c28ba-64f3-48bc-a0a7-7d29b807be1a))
    (pad "16" smd rect (at -5.715 12.5) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "unconnected-(U1-Pad16)") (pinfunction "IO46") (pintype "bidirectional+no_connect") (tstamp 38729c0c-68e9-4494-ab9c-826923dbbea2))
    (pad "17" smd rect (at -4.445 12.5) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 28 "unconnected-(U1-Pad17)") (pinfunction "IO9") (pintype "bidirectional+no_connect") (tstamp 2fab2b84-fb7e-41af-8240-b84fb0258617))
    (pad "18" smd rect (at -3.175 12.5) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "unconnected-(U1-Pad18)") (pinfunction "IO10") (pintype "bidirectional+no_connect") (tstamp 5a569aa4-2223-4cd9-b6a6-c806d050d666))
    (pad "19" smd rect (at -1.905 12.5) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "unconnected-(U1-Pad19)") (pinfunction "IO11") (pintype "bidirectional+no_connect") (tstamp 927b5621-e38a-4729-bd2f-3b47adead4ad))
    (pad "20" smd rect (at -0.635 12.5) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "unconnected-(U1-Pad20)") (pinfunction "IO12") (pintype "bidirectional+no_connect") (tstamp 1447090c-2371-4055-a979-fbfdf7da02f9))
    (pad "21" smd rect (at 0.635 12.5) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "unconnected-(U1-Pad21)") (pinfunction "IO13") (pintype "bidirectional+no_connect") (tstamp d55d7460-ac17-4d21-a1c0-47d7db58221e))
    (pad "22" smd rect (at 1.905 12.5) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "unconnected-(U1-Pad22)") (pinfunction "IO14") (pintype "bidirectional+no_connect") (tstamp e9ef3754-a630-4985-9388-fefd9ce8c704))
    (pad "23" smd rect (at 3.175 12.5) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "unconnected-(U1-Pad23)") (pinfunction "IO21") (pintype "bidirectional+no_connect") (tstamp 81337a78-717f-48e9-99bb-53f3f5ab23ac))
    (pad "24" smd rect (at 4.445 12.5) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "unconnected-(U1-Pad24)") (pinfunction "IO47") (pintype "bidirectional+no_connect") (tstamp 46543ac7-739e-4006-8168-29e022239060))
    (pad "25" smd rect (at 5.715 12.5) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "unconnected-(U1-Pad25)") (pinfunction "IO48") (pintype "bidirectional+no_connect") (tstamp d5ceeef8-408c-48cf-be7a-55060271a0f2))
    (pad "26" smd rect (at 6.985 12.5) (size 0.9 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "unconnected-(U1-Pad26)") (pinfunction "IO45") (pintype "bidirectional+no_connect") (tstamp 9aead608-bf70-4a35-8b50-e4f2c62a1c0e))
    (pad "27" smd rect (at 8.75 11.25) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "IO0") (pinfunction "IO0") (pintype "bidirectional") (tstamp 00fdbe8b-067f-4715-865d-e03cac556258))
    (pad "28" smd rect (at 8.75 9.98) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "unconnected-(U1-Pad28)") (pinfunction "IO35") (pintype "bidirectional+no_connect") (tstamp 730dee08-9a00-4444-9045-e9100fbe6a45))
    (pad "29" smd rect (at 8.75 8.71) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "unconnected-(U1-Pad29)") (pinfunction "IO36") (pintype "bidirectional+no_connect") (tstamp bae72248-d68c-4ba5-86d6-6ae7869481c0))
    (pad "30" smd rect (at 8.75 7.44) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "unconnected-(U1-Pad30)") (pinfunction "IO37") (pintype "bidirectional+no_connect") (tstamp f5a7d0d7-4f32-4f5c-b880-c794f4e3df2e))
    (pad "31" smd rect (at 8.75 6.17) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "unconnected-(U1-Pad31)") (pinfunction "IO38") (pintype "bidirectional+no_connect") (tstamp 298350cc-9fd8-4487-8f20-4d016c3f2d9d))
    (pad "32" smd rect (at 8.75 4.9) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "unconnected-(U1-Pad32)") (pinfunction "IO39") (pintype "bidirectional+no_connect") (tstamp 0b8d24ec-fea1-4e4d-be01-851b6aadf9b9))
    (pad "33" smd rect (at 8.75 3.63) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "unconnected-(U1-Pad33)") (pinfunction "IO40") (pintype "bidirectional+no_connect") (tstamp 8dda56ba-7a46-44d0-966f-82f539613af7))
    (pad "34" smd rect (at 8.75 2.36) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "unconnected-(U1-Pad34)") (pinfunction "IO41") (pintype "bidirectional+no_connect") (tstamp d44ba604-18ca-4b38-9abc-bad7bdc69897))
    (pad "35" smd rect (at 8.75 1.09) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "unconnected-(U1-Pad35)") (pinfunction "IO42") (pintype "bidirectional+no_connect") (tstamp a27e1511-f57b-4381-bd4e-cd92e90c7c38))
    (pad "36" smd rect (at 8.75 -0.18) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "RX0") (pinfunction "RXD0") (pintype "bidirectional") (tstamp e645e73a-ff8b-4302-bac1-19714230d359))
    (pad "37" smd rect (at 8.75 -1.45) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "TX0") (pinfunction "TXD0") (pintype "bidirectional") (tstamp f3224517-4767-4c96-9473-6dd4796f7181))
    (pad "38" smd rect (at 8.75 -2.72) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "unconnected-(U1-Pad38)") (pinfunction "IO2") (pintype "bidirectional+no_connect") (tstamp 996aa0be-2522-46ea-9d8a-1bf8c14e5665))
    (pad "39" smd rect (at 8.75 -3.99) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "unconnected-(U1-Pad39)") (pinfunction "IO1") (pintype "bidirectional+no_connect") (tstamp de129344-af4d-4364-b2eb-ec9fe3bca0fd))
    (pad "40" smd rect (at 8.75 -5.26) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 81954afb-70b9-43bd-a686-e1daa4cc29b8))
    (pad "41_1" smd rect (at -1.5 2.46) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 7cd8cf07-07f2-4063-be24-88dcf3e164d3))
    (pad "41_2" smd rect (at -2.9 2.46) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 2b8afcbc-fb07-4622-9b47-81b094e58a11))
    (pad "41_3" smd rect (at -0.1 2.46) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 4988f287-b1b6-469b-b207-0448c8f1e1b5))
    (pad "41_4" smd rect (at -2.9 3.86) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 70d14339-09db-4bdf-afb8-6c6ef56ac771))
    (pad "41_5" smd rect (at -1.5 3.86) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 24ec3766-ca0b-42d5-9936-fa58442c3178))
    (pad "41_6" smd rect (at -0.1 3.86) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp 29851a89-4640-4f54-a682-cf8e2d7f765d))
    (pad "41_7" smd rect (at -2.9 1.06) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp f0e77914-1d83-4159-be8f-981fd72e98f0))
    (pad "41_8" smd rect (at -1.5 1.06) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp ff760066-3f54-4c0f-80a7-2be5ff6c053a))
    (pad "41_9" smd rect (at -0.1 1.06) (size 0.9 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp cc4757c4-231c-4177-9340-54ecb22d0e86))
    (pad "41_10" thru_hole circle (at -1.5 1.76) (size 0.4 0.4) (drill 0.2) (layers *.Cu) (tstamp efbb6add-2cb3-4e63-bea2-a64e4e290009))
    (pad "41_11" thru_hole circle (at -2.9 1.76) (size 0.4 0.4) (drill 0.2) (layers *.Cu) (tstamp 828f1afd-2255-4dfd-a422-a41e2e673ccd))
    (pad "41_12" thru_hole circle (at -0.1 1.76) (size 0.4 0.4) (drill 0.2) (layers *.Cu) (tstamp 7db0d0ba-ced1-467b-96ab-87258c8071fe))
    (pad "41_13" thru_hole circle (at -2.9 3.16) (size 0.4 0.4) (drill 0.2) (layers *.Cu) (tstamp 12d94e7e-074a-4d55-b0cb-a8aaa77598b4))
    (pad "41_14" thru_hole circle (at -1.5 3.16) (size 0.4 0.4) (drill 0.2) (layers *.Cu) (tstamp 59f261f5-4602-4b36-a333-a4cace12392c))
    (pad "41_15" thru_hole circle (at -0.1 3.16) (size 0.4 0.4) (drill 0.2) (layers *.Cu) (tstamp ab0945c0-219d-4d23-9182-e232dedddc39))
    (pad "41_16" thru_hole circle (at -2.2 1.06) (size 0.4 0.4) (drill 0.2) (layers *.Cu) (tstamp 8d37bfcf-7e30-4e7d-a852-cfe9b0918c5f))
    (pad "41_17" thru_hole circle (at -0.8 1.06) (size 0.4 0.4) (drill 0.2) (layers *.Cu) (tstamp 9b280183-62c1-4247-bb07-cb8257e54961))
    (pad "41_18" thru_hole circle (at -2.2 2.46) (size 0.4 0.4) (drill 0.2) (layers *.Cu) (tstamp ec072509-5854-49ff-8c81-c47d9b3e8360))
    (pad "41_19" thru_hole circle (at -0.8 2.46) (size 0.4 0.4) (drill 0.2) (layers *.Cu) (tstamp de200c0d-fac4-471e-ba5e-d78b4497a2f6))
    (pad "41_20" thru_hole circle (at -2.2 3.86) (size 0.4 0.4) (drill 0.2) (layers *.Cu) (tstamp 155975e7-81fe-4228-943f-3a7a772e603e))
    (pad "41_21" thru_hole circle (at -0.8 3.86) (size 0.4 0.4) (drill 0.2) (layers *.Cu) (tstamp 14c38809-8e38-4fa3-8a1a-a20d52056c75))
    (zone (net 0) (net_name "") (layer "F.Cu") (tstamp c29e9b14-0c62-4ba9-8c5c-a9609ea27376) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.817 67.224)
          (xy 137.817 67.224)
          (xy 137.817 73.224)
          (xy 119.817 73.224)
        )
      )
    )
    (zone (net 0) (net_name "") (layers *.Cu) (tstamp e095884f-0c5a-4624-bb38-05d3e7608383) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks allowed) (vias not_allowed) (pads allowed) (copperpour allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.817 67.224)
          (xy 137.817 67.224)
          (xy 137.817 73.224)
          (xy 119.817 73.224)
        )
      )
    )
    (zone (net 0) (net_name "") (layer "B.Cu") (tstamp 79bd8dde-10c3-4f05-a35f-9502b72d9cc2) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.01)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 119.817 67.224)
          (xy 137.817 67.224)
          (xy 137.817 73.224)
          (xy 119.817 73.224)
        )
      )
    )
    (model "C:/Users/gameb/Desktop/Eskate_Remote/lib/esp32S3/ESP32-S3-WROOM-1-N16R2.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )

  (footprint "USB-C better:GCT_USB4105-GF-A" (layer "F.Cu")
    (tedit 63E00378) (tstamp d0804af9-7a29-401e-9e64-f099632c457c)
    (at 169.164 76.454)
    (property "MANUFACTURER" "GCT")
    (property "MAXIMUM_PACKAGE_HEIGHT" "3.31 mm")
    (property "PARTREV" "A3")
    (property "STANDARD" "Manufacturer Recommendations")
    (property "Sheetfile" "main jednotka.kicad_sch")
    (property "Sheetname" "")
    (path "/f6eaf490-9e1f-4897-969d-df83858b4bab")
    (attr smd)
    (fp_text reference "J1" (at -1.825 -8.135) (layer "F.SilkS")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7c92ccd4-3e1a-4fc0-9ff1-0d0ecb9ca6bb)
    )
    (fp_text value "USB4105-GF-A" (at 5.16 -6.635) (layer "F.Fab")
      (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bddf0143-e19c-49d1-85e5-5b2e1b7f8f1b)
    )
    (fp_text user "PCB EDGE" (at 5.4 2.5) (layer "F.Fab")
      (effects (font (size 0.32 0.32) (thickness 0.15)))
      (tstamp 65c6c8a2-cad5-48b2-a909-7469083c8414)
    )
    (fp_line (start -4.79 1.32) (end -4.79 2.6) (layer "F.SilkS") (width 0.2) (tstamp 15c43e57-8728-4a94-800f-e3ca6f8472cb))
    (fp_line (start 4.79 2.6) (end 4.79 1.32) (layer "F.SilkS") (width 0.2) (tstamp 40296631-9f2b-4cfe-b947-aa945eb0bc8c))
    (fp_line (start -4.79 -2.65) (end -4.79 -1.4) (layer "F.SilkS") (width 0.2) (tstamp 60ce989d-bca8-483f-b07c-d17b4180477e))
    (fp_line (start -4.79 2.6) (end 4.79 2.6) (layer "F.SilkS") (width 0.2) (tstamp 6d454d12-cb82-46ca-9283-b17b3a041c74))
    (fp_line (start 4.79 -2.65) (end 4.79 -1.4) (layer "F.SilkS") (width 0.2) (tstamp a082d3fb-70a1-4a52-a145-b74809a1fab7))
    (fp_line (start -5.1 -5.58) (end -5.1 2.85) (layer "F.CrtYd") (width 0.05) (tstamp 63c19cc2-52a1-4cd7-8768-194fc551dbeb))
    (fp_line (start 5.1 2.85) (end 5.1 -5.58) (layer "F.CrtYd") (width 0.05) (tstamp 658ce583-f210-4290-a037-956c5e9e504f))
    (fp_line (start -5.1 2.85) (end 5.1 2.85) (layer "F.CrtYd") (width 0.05) (tstamp 87ce7bb9-158d-44a5-87fd-0d0166309429))
    (fp_line (start 5.1 -5.58) (end -5.1 -5.58) (layer "F.CrtYd") (width 0.05) (tstamp f758134f-fdf5-4282-9259-f1e5e4c16866))
    (fp_line (start -4.79 2.6) (end -4.79 -4.93) (layer "F.Fab") (width 0.1) (tstamp 05eb78fe-129e-4dcc-908b-154f5d8b52e0))
    (fp_line (start -4.79 -4.93) (end 4.79 -4.93) (layer "F.Fab") (width 0.1) (tstamp 0cd13e41-c969-42bf-9027-9fd0c8cf46ad))
    (fp_line (start 4.79 2.6) (end -4.79 2.6) (layer "F.Fab") (width 0.1) (tstamp 1510d51c-fc4f-4c39-9c25-06efcbfa4adc))
    (fp_line (start 4.8 2.6) (end 8.4 2.6) (layer "F.Fab") (width 0.1) (tstamp 4095d957-ffc9-4ca3-af63-a3ae74d51a7e))
    (fp_line (start 4.79 -4.93) (end 4.79 2.6) (layer "F.Fab") (width 0.1) (tstamp f115db0e-52f6-4fb5-8193-8a30aa75abb2))
    (pad "" np_thru_hole circle (at -2.89 -3.68) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask) (tstamp b43037e6-5b2c-4b4c-8e47-ff80553f6e69))
    (pad "" np_thru_hole circle (at 2.89 -3.68) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask) (tstamp dc94ffee-a5f8-43bf-8161-5ae740fdcc60))
    (pad "A1_B12" smd rect (at -3.2 -4.755) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(J1-PadA1_B12)") (pinfunction "GND") (pintype "power_in") (tstamp 2a226be3-851f-4de8-9be5-c7b8347b2230))
    (pad "A4_B9" smd rect (at -2.4 -4.755) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(J1-PadA4_B9)") (pinfunction "VBUS") (pintype "power_in") (tstamp ef9bea4b-d244-4fc1-836f-735f3a12cad9))
    (pad "A5" smd rect (at -1.25 -4.755) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "unconnected-(J1-PadA5)") (pinfunction "CC1") (pintype "bidirectional") (tstamp 80322bb4-8a99-4ca8-a3c8-2a299d07fbb5))
    (pad "A6" smd rect (at -0.25 -4.755) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "unconnected-(J1-PadA6)") (pinfunction "DP1") (pintype "bidirectional") (tstamp e77454e8-a515-41a7-b10e-c24fc17720f1))
    (pad "A7" smd rect (at 0.25 -4.755) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "unconnected-(J1-PadA7)") (pinfunction "DN1") (pintype "bidirectional") (tstamp ba7e7157-76ba-410b-b195-c8b38dde4e51))
    (pad "A8" smd rect (at 1.25 -4.755) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "unconnected-(J1-PadA8)") (pinfunction "SBU1") (pintype "bidirectional") (tstamp 226df6fc-0740-41a4-ab2c-4e8a3817f635))
    (pad "B1_A12" smd rect (at 3.2 -4.755) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(J1-PadA1_B12)") (pinfunction "GND") (pintype "power_in") (tstamp 5bfe88f6-f111-4d62-923b-04d96a05850b))
    (pad "B4_A9" smd rect (at 2.4 -4.755) (size 0.6 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(J1-PadA4_B9)") (pinfunction "VBUS") (pintype "power_in") (tstamp 493f0865-9df4-4b23-ac47-2817770e17d0))
    (pad "B5" smd rect (at 1.75 -4.755) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "unconnected-(J1-PadB5)") (pinfunction "CC2") (pintype "bidirectional") (tstamp 9265f274-02af-4bc2-8409-fe2baaf877a4))
    (pad "B6" smd rect (at 0.75 -4.755) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "unconnected-(J1-PadB6)") (pinfunction "DP2") (pintype "bidirectional") (tstamp f97b5d0f-7889-4526-902c-295bbde833bf))
    (pad "B7" smd rect (at -0.75 -4.755) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "unconnected-(J1-PadB7)") (pinfunction "DN2") (pintype "bidirectional") (tstamp 46da5df3-e800-45cd-a208-da288aa8d49d))
    (pad "B8" smd rect (at -1.75 -4.755) (size 0.3 1.15) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "unconnected-(J1-PadB8)") (pinfunction "SBU2") (pintype "bidirectional") (tstamp 9a4d451c-dd4d-4313-9007-9a21ab87398b))
    (pad "S1" thru_hole oval (at -4.32 -4.18) (size 1.05 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-PadS1)") (pinfunction "SHELL_GND") (pintype "power_in") (tstamp 632b4c4a-8dbb-4ba1-bd6f-3469de95d82b))
    (pad "S2" thru_hole oval (at -4.32 0) (size 1 2) (drill oval 0.6 1.4) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-PadS1)") (pinfunction "SHELL_GND") (pintype "power_in") (tstamp b39fe6cd-dda4-4b38-9346-b521b721b7b6))
    (pad "S3" thru_hole oval (at 4.32 0) (size 1 2) (drill oval 0.6 1.4) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-PadS1)") (pinfunction "SHELL_GND") (pintype "power_in") (tstamp 0c65b59e-8f2d-4f38-aa33-c6bf72d7196e))
    (pad "S4" thru_hole oval (at 4.32 -4.18) (size 1.05 2.1) (drill oval 0.6 1.7) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-PadS1)") (pinfunction "SHELL_GND") (pintype "power_in") (tstamp 7b874a17-6d78-4844-8348-f0c5323c01e4))
    (model "C:/Users/gameb/Desktop/Eskate_Remote/lib/USB-C better/USB4105-GF-A.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )

)
